|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Competitor |  | **Sail No** |  | **Boat No** |  |  | **ILCA Rig** |
|  |  | | | | | |  |
|  | **Declaration to be signed by competitor**  I have passed measurement and will not change anything on my boat during this series without the permission of the Measurer or Race Committee.  Signed………………………………………………………………… | | | | | |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Lines & Hull** | **Lines** | | **OK** | **Comment** |
| Traveller one line - no multi purchase systems | |  |  |
| Mainsheet one continuous length | |  |  |
| Boom vang 2 lines 7 turn points max | |  |  |
| Outhaul 2 lines 6 turn points max quick release clew hook | |  |  |
| Cunningham 3 lines 5 turn points max | |  |  |
| Pulleys between 15 to 30 mm diameter | |  |  |
| Mast tie down rope | |  |  |
| Centreboard retaining line or shock cord | |  |  |
| **Hull** | | **OK** | **Comment** |
| C/B case clear. Front tape max 30X30X2mm | |  |  |
| Mast step no devices to prevent fore & aft movement | |  |  |
| Hiking strap non-stretch material | |  |  |
| Electronic compliance ILCA Rule 22 - compass, time, heart rate | |  | **Sailing Instructions - 1.4** |
| Boat compliance sticker with number | |  |  |
| **Dolly** | **Dolly** | | **OK** | **Comment** |
| Functional frame, axles, wheels & retaining pins, adequate padding | |  |  |
| **Spars** | **Spars** | **Straight  OK** | **Measurements OK** | **Comment** |
| Bottom section (sleeve ILCA6) |  |  |  |
| Bottom section drain hole open | N/A |  |  |
| Top section |  |  |  |
| Top section watertight | N/A |  |  |
| Boom |  |  |  |
| **Foils & Tiller** | **Foils & Tiller** | | **OK** | **Comment** |
| Rudder thickness 20mm max | |  |  |
| Rudder angle max 78° | |  |  |
| Rudder bolt 10mm washers 20mm dia max | |  |  |
| Rudder downhaul line fitted | |  |  |
| Tiller removable from rudder | |  |  |
| Tiller fitted with rudder cleat | |  |  |
| Centreboard thickness 33mm max | |  |  |
| Centreboard standard stopper assembly fitted | |  |  |
| Centreboard Handle (if fitted) 2 holes max | |  |  |
| **Sail** | **Sail** | | **OK** | **Comment** |
| Button on sail | |  |  |
| Number on sail as per this sheet & national letters fitted | |  |  |
| Numbers size | |  |  |
| Rhombus fitted if female sailor | |  |  |
| Battens length | |  |  |